
T0F10 000:002 SEGGER J-Link V6.52b Log File (0000ms, 0002ms total)
T0F10 000:002 DLL Compiled: Oct  8 2019 12:29:01 (0000ms, 0002ms total)
T0F10 000:002 Logging started @ 2021-04-29 08:39 (0000ms, 0002ms total)
T0F10 000:002 JLINK_SetWarnOutHandler(...) (0000ms, 0002ms total)
T0F10 000:002 JLINK_OpenEx(...)
Firmware: J-Link V9 compiled Dec 13 2019 11:14:50
Hardware: V9.70
S/N: 20781318
Feature(s): GDB, RDI, FlashBP, FlashDL, JFlash, RDDI
TELNET listener socket opened on port 19021WEBSRV 
Starting webserver (0037ms, 0039ms total)
T0F10 000:002 WEBSRV Webserver running on local port 19080 (0037ms, 0039ms total)
T0F10 000:002   returns O.K. (0037ms, 0039ms total)
T0F10 000:039 JLINK_GetEmuCaps()  returns 0xB9FF7BBF (0000ms, 0039ms total)
T0F10 000:039 JLINK_TIF_GetAvailable(...) (0000ms, 0039ms total)
T0F10 000:039 JLINK_SetErrorOutHandler(...) (0000ms, 0039ms total)
T0F10 000:039 JLINK_ExecCommand("ProjectFile = "D:\test\MDK-ARM\JLinkSettings.ini"", ...). Ref file found at: C:\Keil_v5\ARM\Segger\JLinkDevices.ref (0002ms, 0041ms total)
T0F10 000:039 XML referenced by ref file: C:\Program Files (x86)\SEGGER\JLink\JLinkDevices.xml (0002ms, 0041ms total)
T0F10 000:039 C:\Program Files (x86)\SEGGER\JLink\JLinkDevices.xml evaluated successfully. (0004ms, 0043ms total)
T0F10 000:039   returns 0x00 (0147ms, 0186ms total)
T0F10 000:186 JLINK_ExecCommand("Device = STM32F103RC", ...). Device "STM32F103RC" selected.  returns 0x00 (0000ms, 0186ms total)
T0F10 000:186 JLINK_ExecCommand("DisableConnectionTimeout", ...).   returns 0x01 (0000ms, 0186ms total)
T0F10 000:186 JLINK_GetHardwareVersion()  returns 0x17AE8 (0000ms, 0186ms total)
T0F10 000:187 JLINK_GetDLLVersion()  returns 65202 (0000ms, 0186ms total)
T0F10 000:187 JLINK_GetFirmwareString(...)
T0F10 000:187 (0000ms, 0186ms total)
T0F10 000:187 JLINK_GetDLLVersion()  returns 65202 (0000ms, 0186ms total)
T0F10 000:187 JLINK_GetCompileDateTime() (0000ms, 0186ms total)
T0F10 000:187 JLINK_GetFirmwareString(...)
T0F10 000:187 (0000ms, 0186ms total)
T0F10 000:187 JLINK_GetHardwareVersion()  returns 0x17AE8 (0000ms, 0186ms total)
T0F10 000:187 JLINK_TIF_Select(JLINKARM_TIF_SWD)  returns 0x00 (0000ms, 0186ms total)
T0F10 000:187 JLINK_SetSpeed(5000) (0000ms, 0186ms total)
T0F10 000:187 JLINK_GetId()Found SW-DP with ID 0x2BA01477RESET (pin 15) high, but should be low. Please check target hardware.Found SW-DP with ID 0x2BA01477Scanning AP map to find all available APsAP[1]: Stopped AP scan as end of AP map has been reachedAP[0]: AHB-AP (IDR: 0x24770011)Iterating through AP map to find AHB-AP to useAP[0]: Core foundAP[0]: AHB-AP ROM base: 0xE00FF000CPUID register: 0x410FC241. Implementer code: 0x41 (ARM)Found Cortex-M4 r0p1, Little endian.
Identified core does not match configuration. (Found: Cortex-M4, Configured: Cortex-M3) -- Max. mem block: 0x00010D88 -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE0002000)FPUnit: 6 code (BP) slots and 2 literal slots -- CPU_ReadMem(4 bytes @ 0xE000EDFC) -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0001000) -- CPU_ReadMem(4 bytes @ 0xE000ED88) -- CPU_WriteMem(4 bytes @ 0xE000ED88)
 -- CPU_ReadMem(4 bytes @ 0xE000ED88) -- CPU_WriteMem(4 bytes @ 0xE000ED88)CoreSight components:ROMTbl[0] @ E00FF000 -- CPU_ReadMem(16 bytes @ 0xE00FF000) -- CPU_ReadMem(16 bytes @ 0xE000EFF0) -- CPU_ReadMem(16 bytes @ 0xE000EFE0)ROMTbl[0][0]: E000E000, CID: B105E00D, PID: 000BB00C SCS-M7 -- CPU_ReadMem(16 bytes @ 0xE0001FF0) -- CPU_ReadMem(16 bytes @ 0xE0001FE0)ROMTbl[0][1]: E0001000, CID: B105E00D, PID: 003BB002 DWT -- CPU_ReadMem(16 bytes @ 0xE0002FF0) -- CPU_ReadMem(16 bytes @ 0xE0002FE0)
ROMTbl[0][2]: E0002000, CID: B105E00D, PID: 002BB003 FPB -- CPU_ReadMem(16 bytes @ 0xE0000FF0) -- CPU_ReadMem(16 bytes @ 0xE0000FE0)ROMTbl[0][3]: E0000000, CID: B105E00D, PID: 003BB001 ITM -- CPU_ReadMem(16 bytes @ 0xE00FF010) -- CPU_ReadMem(16 bytes @ 0xE0040FF0) -- CPU_ReadMem(16 bytes @ 0xE0040FE0)ROMTbl[0][4]: E0040000, CID: B105900D, PID: 000BB9A1 TPIU -- CPU_ReadMem(16 bytes @ 0xE0041FF0) -- CPU_ReadMem(16 bytes @ 0xE0041FE0)ROMTbl[0][5]: E0041000, CID: B105900D, PID: 000BB925 ETM
  returns 0x2BA01477 (0329ms, 0515ms total)
T0F10 000:516 JLINK_GetDLLVersion()  returns 65202 (0000ms, 0515ms total)
T0F10 000:516 JLINK_CORE_GetFound()  returns 0xE0000FF (0000ms, 0515ms total)
T0F10 000:516 JLINK_GetDebugInfo(0x100 = JLINKARM_ROM_TABLE_ADDR_INDEX) -- Value=0xE00FF000  returns 0x00 (0000ms, 0515ms total)
T0F10 000:516 JLINK_GetDebugInfo(0x100 = JLINKARM_ROM_TABLE_ADDR_INDEX) -- Value=0xE00FF000  returns 0x00 (0000ms, 0515ms total)
T0F10 000:516 JLINK_GetDebugInfo(0x101 = JLINKARM_DEBUG_INFO_ETM_ADDR_INDEX) -- Value=0xE0041000  returns 0x00 (0000ms, 0515ms total)
T0F10 000:516 JLINK_ReadMemEx(0xE0041FD0, 0x0020 Bytes, ..., Flags = 0x02000004) -- CPU_ReadMem(32 bytes @ 0xE0041FD0) - Data: 04 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0001ms, 0516ms total)
T0F10 000:517 JLINK_GetDebugInfo(0x102 = JLINKARM_DEBUG_INFO_MTB_ADDR_INDEX) -- Value=0x00000000  returns 0x00 (0000ms, 0516ms total)
T0F10 000:517 JLINK_GetDebugInfo(0x103 = JLINKARM_DEBUG_INFO_TPIU_ADDR_INDEX) -- Value=0xE0040000  returns 0x00 (0000ms, 0516ms total)
T0F10 000:517 JLINK_GetDebugInfo(0x104 = JLINKARM_DEBUG_INFO_ITM_ADDR_INDEX) -- Value=0xE0000000  returns 0x00 (0000ms, 0516ms total)
T0F10 000:517 JLINK_GetDebugInfo(0x105 = JLINKARM_DEBUG_INFO_DWT_ADDR_INDEX) -- Value=0xE0001000  returns 0x00 (0000ms, 0516ms total)
T0F10 000:517 JLINK_GetDebugInfo(0x106 = JLINKARM_DEBUG_INFO_FPB_ADDR_INDEX) -- Value=0xE0002000  returns 0x00 (0000ms, 0516ms total)
T0F10 000:517 JLINK_GetDebugInfo(0x107 = JLINKARM_DEBUG_INFO_NVIC_ADDR_INDEX) -- Value=0xE000E000  returns 0x00 (0000ms, 0516ms total)
T0F10 000:517 JLINK_GetDebugInfo(0x10C = JLINKARM_DEBUG_INFO_DBG_ADDR_INDEX) -- Value=0xE000EDF0  returns 0x00 (0000ms, 0516ms total)
T0F10 000:517 JLINK_ReadMemU32(0xE000EF40, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000EF40) - Data: 21 00 11 10  returns 1 (0000ms, 0516ms total)
T0F10 000:517 JLINK_ReadMemU32(0xE000EF44, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000EF44) - Data: 11 00 00 11  returns 1 (0000ms, 0516ms total)
T0F10 000:517 JLINK_ReadMemU32(0xE000ED00, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000ED00) - Data: 41 C2 0F 41  returns 1 (0001ms, 0517ms total)
T0F10 000:518 JLINK_GetDebugInfo(0x10F = JLINKARM_DEBUG_INFO_HAS_CORTEX_M_SECURITY_EXT_INDEX) -- Value=0x00000000  returns 0x00 (0000ms, 0517ms total)
T0F10 000:518 JLINK_SetResetType(JLINKARM_CM3_RESET_TYPE_NORMAL)  returns JLINKARM_CM3_RESET_TYPE_NORMAL (0000ms, 0517ms total)
T0F10 000:518 JLINK_Reset() -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDFC)Reset: Halt core after reset via DEMCR.VC_CORERESET.Reset: Reset device via AIRCR.SYSRESETREQ. -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000ED0C) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDFC)
 -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE0002000) -- CPU_ReadMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE0001000) (0064ms, 0581ms total)
T0F10 000:582 JLINK_ReadReg(R15 (PC))  returns 0x080001F0 (0000ms, 0581ms total)
T0F10 000:582 JLINK_ReadReg(XPSR)  returns 0x01000000 (0000ms, 0581ms total)
T0F10 000:582 JLINK_Halt()  returns 0x00 (0000ms, 0581ms total)
T0F10 000:582 JLINK_ReadMemU32(0xE000EDF0, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) - Data: 03 00 03 00  returns 1 (0000ms, 0581ms total)
T0F10 000:582 JLINK_WriteU32(0xE000EDF0, 0xA05F0003) -- CPU_WriteMem(4 bytes @ 0xE000EDF0)  returns 0 (0001ms, 0582ms total)
T0F10 000:583 JLINK_WriteU32(0xE000EDFC, 0x01000000) -- CPU_WriteMem(4 bytes @ 0xE000EDFC)  returns 0 (0000ms, 0582ms total)
T0F10 000:583 JLINK_GetHWStatus(...)  returns 0x00 (0000ms, 0582ms total)
T0F10 000:583 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)  returns 0x06 (0000ms, 0582ms total)
T0F10 000:583 JLINK_GetNumBPUnits(Type = 0xF0)  returns 0x2000 (0000ms, 0582ms total)
T0F10 000:583 JLINK_GetNumWPUnits()  returns 0x04 (0000ms, 0582ms total)
T0F10 000:583 JLINK_GetSpeed()  returns 0xFA0 (0000ms, 0582ms total)
T0F10 000:583 JLINK_ReadMemU32(0xE000E004, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000E004) - Data: 02 00 00 00  returns 1 (0000ms, 0582ms total)
T0F10 000:583 JLINK_ReadMemU32(0xE000E004, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000E004) - Data: 02 00 00 00  returns 1 (0001ms, 0583ms total)
T0F10 000:584 JLINK_WriteMemEx(0xE0001000, 0x001C Bytes, ..., Flags = 0x02000004) - Data: 01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ... -- CPU_WriteMem(28 bytes @ 0xE0001000)  returns 0x1C (0002ms, 0585ms total)
T0F10 000:586 JLINK_ReadReg(R15 (PC))  returns 0x080001F0 (0000ms, 0585ms total)
T0F10 000:586 JLINK_ReadReg(XPSR)  returns 0x01000000 (0000ms, 0585ms total)
T0F10 000:692 JLINK_SetResetType(JLINKARM_CM3_RESET_TYPE_NORMAL)  returns JLINKARM_CM3_RESET_TYPE_NORMAL (0000ms, 0585ms total)
T0F10 000:692 JLINK_Reset() -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDFC)Reset: Halt core after reset via DEMCR.VC_CORERESET.Reset: Reset device via AIRCR.SYSRESETREQ. -- CPU_WriteMem(4 bytes @ 0xE000ED0C) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE0002000) -- CPU_ReadMem(4 bytes @ 0xE000EDFC)
 -- CPU_ReadMem(4 bytes @ 0xE0001000) (0065ms, 0650ms total)
T0F10 000:757 JLINK_ReadReg(R15 (PC))  returns 0x080001F0 (0000ms, 0650ms total)
T0F10 000:757 JLINK_ReadReg(XPSR)  returns 0x01000000 (0000ms, 0650ms total)
T0F10 000:758 JLINK_ReadMemEx(0x080001F0, 0x003C Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(128 bytes @ 0x080001C0) -- Updating C cache (128 bytes @ 0x080001C0) -- Read from C cache (60 bytes @ 0x080001F0) - Data: 09 48 80 47 09 48 00 47 FE E7 FE E7 FE E7 FE E7 ...  returns 0x3C (0001ms, 0651ms total)
T0F10 001:854 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 0651ms total)
T0F10 001:854 JLINK_ReadReg(R1)  returns 0x00000000 (0000ms, 0651ms total)
T0F10 001:854 JLINK_ReadReg(R2)  returns 0x00000000 (0000ms, 0651ms total)
T0F10 001:854 JLINK_ReadReg(R3)  returns 0x00000000 (0000ms, 0651ms total)
T0F10 001:854 JLINK_ReadReg(R4)  returns 0x00000000 (0000ms, 0651ms total)
T0F10 001:854 JLINK_ReadReg(R5)  returns 0x00000000 (0000ms, 0651ms total)
T0F10 001:854 JLINK_ReadReg(R6)  returns 0x00000000 (0000ms, 0651ms total)
T0F10 001:854 JLINK_ReadReg(R7)  returns 0x00000000 (0000ms, 0651ms total)
T0F10 001:854 JLINK_ReadReg(R8)  returns 0x00000000 (0000ms, 0651ms total)
T0F10 001:854 JLINK_ReadReg(R9)  returns 0x00000000 (0000ms, 0651ms total)
T0F10 001:854 JLINK_ReadReg(R10)  returns 0x00000000 (0000ms, 0651ms total)
T0F10 001:854 JLINK_ReadReg(R11)  returns 0x00000000 (0000ms, 0651ms total)
T0F10 001:854 JLINK_ReadReg(R12)  returns 0x00000000 (0000ms, 0651ms total)
T0F10 001:854 JLINK_ReadReg(R13 (SP))  returns 0x20000FA8 (0000ms, 0651ms total)
T0F10 001:854 JLINK_ReadReg(R14)  returns 0xFFFFFFFF (0000ms, 0651ms total)
T0F10 001:854 JLINK_ReadReg(R15 (PC))  returns 0x080001F0 (0000ms, 0651ms total)
T0F10 001:854 JLINK_ReadReg(XPSR)  returns 0x01000000 (0000ms, 0651ms total)
T0F10 001:854 JLINK_ReadReg(MSP)  returns 0x20000FA8 (0000ms, 0651ms total)
T0F10 001:854 JLINK_ReadReg(PSP)  returns 0x00000000 (0000ms, 0651ms total)
T0F10 001:854 JLINK_ReadReg(CFBP)  returns 0x00000000 (0000ms, 0651ms total)
T0F10 001:854 JLINK_ReadReg(FPSCR)  returns 0x00000000 (0003ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS0)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS1)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS2)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS3)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS4)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS5)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS6)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS7)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS8)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS9)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS10)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS11)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS12)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS13)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS14)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS15)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS16)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS17)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS18)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS19)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS20)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS21)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS22)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS23)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS24)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS25)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS26)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS27)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS28)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS29)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS30)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:857 JLINK_ReadReg(FPS31)  returns 0x00000000 (0000ms, 0654ms total)
T0F10 001:867 JLINK_ReadMemEx(0x200029D0, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(64 bytes @ 0x200029C0) -- Updating C cache (64 bytes @ 0x200029C0) -- Read from C cache (32 bytes @ 0x200029D0) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0000ms, 0654ms total)
T0F10 001:875 JLINK_ReadMemEx(0x200002A0, 0x0004 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(64 bytes @ 0x20000280) -- Updating C cache (64 bytes @ 0x20000280) -- Read from C cache (4 bytes @ 0x200002A0) - Data: 00 00 00 00  returns 0x04 (0001ms, 0655ms total)
T0F10 001:880 JLINK_ReadMemEx(0x20000E60, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(64 bytes @ 0x20000E40) -- Updating C cache (64 bytes @ 0x20000E40) -- Read from C cache (32 bytes @ 0x20000E60) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0001ms, 0656ms total)
T0F10 001:894 JLINK_ReadMemEx(0x00000000, 0x0001 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(4 bytes @ 0x40023844) -- CPU_ReadMem(64 bytes @ 0x08000000) -- Updating C cache (64 bytes @ 0x08000000) -- Read from C cache (1 bytes @ 0x08000000) - Data: A8  returns 0x01 (0001ms, 0657ms total)
T0F10 001:895 JLINK_ReadMemEx(0x2000029F, 0x0001 Bytes, ..., Flags = 0x02000000) -- Read from C cache (1 bytes @ 0x2000029F) - Data: 00  returns 0x01 (0000ms, 0657ms total)
T27A0 001:916 JLINK_ReadMemEx(0x080001F0, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x080001F0) - Data: 09 48  returns 0x02 (0000ms, 0657ms total)
T27A0 001:916 JLINK_SetBPEx(Addr = 0x08002AAE, Type = 0xFFFFFFF2)  returns 0x00000001 (0000ms, 0657ms total)
T27A0 001:916 JLINK_Go() -- CPU_WriteMem(4 bytes @ 0xE0002000) -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) -- CPU_WriteMem(4 bytes @ 0xE0001004) (0002ms, 0659ms total)
T27A0 002:019 JLINK_IsHalted()  returns FALSE (0000ms, 0659ms total)
T27A0 002:120 JLINK_IsHalted()  returns TRUE (0001ms, 0660ms total)
T27A0 002:121 JLINK_Halt()  returns 0x00 (0000ms, 0659ms total)
T27A0 002:121 JLINK_IsHalted()  returns TRUE (0000ms, 0659ms total)
T27A0 002:121 JLINK_IsHalted()  returns TRUE (0000ms, 0659ms total)
T27A0 002:121 JLINK_IsHalted()  returns TRUE (0000ms, 0659ms total)
T27A0 002:121 JLINK_ReadReg(R15 (PC))  returns 0x08002AAE (0001ms, 0660ms total)
T27A0 002:122 JLINK_ReadReg(XPSR)  returns 0x61000000 (0000ms, 0660ms total)
T27A0 002:122 JLINK_ClrBPEx(BPHandle = 0x00000001)  returns 0x00 (0000ms, 0660ms total)
T27A0 002:122 JLINK_ReadMemU32(0xE000ED30, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000ED30) - Data: 02 00 00 00  returns 1 (0000ms, 0660ms total)
T27A0 002:122 JLINK_ReadMemU32(0xE0001028, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001028) - Data: 00 00 00 00  returns 1 (0000ms, 0660ms total)
T27A0 002:122 JLINK_ReadMemU32(0xE0001038, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001038) - Data: 00 02 00 00  returns 1 (0001ms, 0661ms total)
T27A0 002:123 JLINK_ReadMemU32(0xE0001048, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001048) - Data: 00 00 00 00  returns 1 (0000ms, 0661ms total)
T27A0 002:123 JLINK_ReadMemU32(0xE0001058, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001058) - Data: 00 00 00 00  returns 1 (0000ms, 0661ms total)
T27A0 002:123 JLINK_ReadReg(R0)  returns 0x08002AAF (0000ms, 0661ms total)
T27A0 002:123 JLINK_ReadReg(R1)  returns 0x2000BA70 (0000ms, 0661ms total)
T27A0 002:123 JLINK_ReadReg(R2)  returns 0x00000000 (0000ms, 0661ms total)
T27A0 002:123 JLINK_ReadReg(R3)  returns 0x08008A01 (0000ms, 0661ms total)
T27A0 002:123 JLINK_ReadReg(R4)  returns 0x0801121C (0000ms, 0661ms total)
T27A0 002:123 JLINK_ReadReg(R5)  returns 0x0801121C (0000ms, 0661ms total)
T27A0 002:123 JLINK_ReadReg(R6)  returns 0x00000000 (0000ms, 0661ms total)
T27A0 002:123 JLINK_ReadReg(R7)  returns 0x00000000 (0000ms, 0661ms total)
T27A0 002:123 JLINK_ReadReg(R8)  returns 0x00000000 (0000ms, 0661ms total)
T27A0 002:123 JLINK_ReadReg(R9)  returns 0x00000000 (0000ms, 0661ms total)
T27A0 002:123 JLINK_ReadReg(R10)  returns 0x08001A18 (0000ms, 0661ms total)
T27A0 002:123 JLINK_ReadReg(R11)  returns 0x00000000 (0000ms, 0661ms total)
T27A0 002:123 JLINK_ReadReg(R12)  returns 0x00000004 (0000ms, 0661ms total)
T27A0 002:123 JLINK_ReadReg(R13 (SP))  returns 0x2000BA70 (0000ms, 0661ms total)
T27A0 002:123 JLINK_ReadReg(R14)  returns 0x08002A51 (0000ms, 0661ms total)
T27A0 002:123 JLINK_ReadReg(R15 (PC))  returns 0x08002AAE (0000ms, 0661ms total)
T27A0 002:123 JLINK_ReadReg(XPSR)  returns 0x61000000 (0000ms, 0661ms total)
T27A0 002:123 JLINK_ReadReg(MSP)  returns 0x2000BA70 (0000ms, 0661ms total)
T27A0 002:123 JLINK_ReadReg(PSP)  returns 0x00000000 (0000ms, 0661ms total)
T27A0 002:123 JLINK_ReadReg(CFBP)  returns 0x00000000 (0000ms, 0661ms total)
T27A0 002:123 JLINK_ReadReg(FPSCR)  returns 0x00000000 (0003ms, 0664ms total)
T27A0 002:126 JLINK_ReadReg(FPS0)  returns 0x00000000 (0000ms, 0664ms total)
T27A0 002:126 JLINK_ReadReg(FPS1)  returns 0x00000000 (0000ms, 0664ms total)
T27A0 002:126 JLINK_ReadReg(FPS2)  returns 0x00000000 (0000ms, 0664ms total)
T27A0 002:126 JLINK_ReadReg(FPS3)  returns 0x00000000 (0000ms, 0664ms total)
T27A0 002:126 JLINK_ReadReg(FPS4)  returns 0x00000000 (0000ms, 0664ms total)
T27A0 002:126 JLINK_ReadReg(FPS5)  returns 0x00000000 (0000ms, 0664ms total)
T27A0 002:126 JLINK_ReadReg(FPS6)  returns 0x00000000 (0000ms, 0664ms total)
T27A0 002:126 JLINK_ReadReg(FPS7)  returns 0x00000000 (0001ms, 0665ms total)
T27A0 002:127 JLINK_ReadReg(FPS8)  returns 0x00000000 (0000ms, 0665ms total)
T27A0 002:127 JLINK_ReadReg(FPS9)  returns 0x00000000 (0000ms, 0665ms total)
T27A0 002:127 JLINK_ReadReg(FPS10)  returns 0x00000000 (0000ms, 0665ms total)
T27A0 002:127 JLINK_ReadReg(FPS11)  returns 0x00000000 (0000ms, 0665ms total)
T27A0 002:127 JLINK_ReadReg(FPS12)  returns 0x00000000 (0000ms, 0665ms total)
T27A0 002:127 JLINK_ReadReg(FPS13)  returns 0x00000000 (0000ms, 0665ms total)
T27A0 002:127 JLINK_ReadReg(FPS14)  returns 0x00000000 (0000ms, 0665ms total)
T27A0 002:127 JLINK_ReadReg(FPS15)  returns 0x00000000 (0000ms, 0665ms total)
T27A0 002:127 JLINK_ReadReg(FPS16)  returns 0x00000000 (0000ms, 0665ms total)
T27A0 002:127 JLINK_ReadReg(FPS17)  returns 0x00000000 (0000ms, 0665ms total)
T27A0 002:127 JLINK_ReadReg(FPS18)  returns 0x00000000 (0000ms, 0665ms total)
T27A0 002:127 JLINK_ReadReg(FPS19)  returns 0x00000000 (0000ms, 0665ms total)
T27A0 002:127 JLINK_ReadReg(FPS20)  returns 0x00000000 (0000ms, 0665ms total)
T27A0 002:127 JLINK_ReadReg(FPS21)  returns 0x00000000 (0000ms, 0665ms total)
T27A0 002:127 JLINK_ReadReg(FPS22)  returns 0x00000000 (0000ms, 0665ms total)
T27A0 002:127 JLINK_ReadReg(FPS23)  returns 0x00000000 (0000ms, 0665ms total)
T27A0 002:127 JLINK_ReadReg(FPS24)  returns 0x00000000 (0000ms, 0665ms total)
T27A0 002:127 JLINK_ReadReg(FPS25)  returns 0x00000000 (0000ms, 0665ms total)
T27A0 002:127 JLINK_ReadReg(FPS26)  returns 0x00000000 (0000ms, 0665ms total)
T27A0 002:127 JLINK_ReadReg(FPS27)  returns 0x00000000 (0000ms, 0665ms total)
T27A0 002:127 JLINK_ReadReg(FPS28)  returns 0x00000000 (0000ms, 0665ms total)
T27A0 002:127 JLINK_ReadReg(FPS29)  returns 0x00000000 (0000ms, 0665ms total)
T27A0 002:127 JLINK_ReadReg(FPS30)  returns 0x00000000 (0000ms, 0665ms total)
T27A0 002:127 JLINK_ReadReg(FPS31)  returns 0x00000000 (0000ms, 0665ms total)
T0F10 002:127 JLINK_ReadMemEx(0x200029D0, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(64 bytes @ 0x200029C0) -- Updating C cache (64 bytes @ 0x200029C0) -- Read from C cache (32 bytes @ 0x200029D0) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0001ms, 0666ms total)
T0F10 002:129 JLINK_ReadMemEx(0x200002A0, 0x0004 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(64 bytes @ 0x20000280) -- Updating C cache (64 bytes @ 0x20000280) -- Read from C cache (4 bytes @ 0x200002A0) - Data: 00 00 00 00  returns 0x04 (0000ms, 0666ms total)
T0F10 002:130 JLINK_ReadMemEx(0x20000E60, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(64 bytes @ 0x20000E40) -- Updating C cache (64 bytes @ 0x20000E40) -- Read from C cache (32 bytes @ 0x20000E60) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0000ms, 0666ms total)
T0F10 002:130 JLINK_ReadMemEx(0x08002AAE, 0x0002 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(64 bytes @ 0x08002A80) -- Updating C cache (64 bytes @ 0x08002A80) -- Read from C cache (2 bytes @ 0x08002AAE) - Data: 10 B5  returns 0x02 (0001ms, 0667ms total)
T0F10 002:131 JLINK_ReadMemEx(0x08002AB0, 0x003C Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(64 bytes @ 0x08002AC0) -- Updating C cache (64 bytes @ 0x08002AC0) -- Read from C cache (60 bytes @ 0x08002AB0) - Data: 0B F0 75 FE 00 20 10 BD 30 B5 16 49 16 4B 0A 46 ...  returns 0x3C (0000ms, 0667ms total)
T27A0 003:311 JLINK_ReadMemEx(0x08002AAE, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08002AAE) - Data: 10 B5  returns 0x02 (0000ms, 0667ms total)
T27A0 003:311 JLINK_Go() -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0002008) (0001ms, 0668ms total)
T27A0 003:412 JLINK_IsHalted()  returns FALSE (0000ms, 0668ms total)
T27A0 003:513 JLINK_IsHalted()  returns FALSE (0000ms, 0668ms total)
T27A0 003:614 JLINK_IsHalted()  returns FALSE (0000ms, 0668ms total)
T27A0 003:715 JLINK_IsHalted()  returns FALSE (0001ms, 0669ms total)
T27A0 003:816 JLINK_IsHalted()  returns FALSE (0000ms, 0668ms total)
T27A0 003:917 JLINK_ReadMemU32(0xE0001004, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001004) - Data: 4D CC 74 03  returns 1 (0000ms, 0668ms total)
T0F10 003:917 JLINK_ReadMemEx(0x200029D0, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x200029D0) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0001ms, 0669ms total)
T0F10 003:919 JLINK_ReadMemEx(0x200002A0, 0x0004 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(4 bytes @ 0x200002A0) - Data: 00 00 00 00  returns 0x04 (0001ms, 0670ms total)
T0F10 003:920 JLINK_ReadMemEx(0x20000E60, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x20000E60) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0000ms, 0670ms total)
T27A0 003:920 JLINK_IsHalted()  returns FALSE (0001ms, 0671ms total)
T27A0 004:022 JLINK_IsHalted()  returns FALSE (0000ms, 0670ms total)
T27A0 004:122 JLINK_IsHalted()  returns FALSE (0000ms, 0670ms total)
T27A0 004:223 JLINK_IsHalted()  returns FALSE (0000ms, 0670ms total)
T27A0 004:325 JLINK_IsHalted()  returns FALSE (0000ms, 0670ms total)
T27A0 004:426 JLINK_ReadMemU32(0xE0001004, 0x0001 Items, ...) - Data: 4D CC 74 03  returns 1 (0000ms, 0670ms total)
T0F10 004:426 JLINK_ReadMemEx(0x200029D0, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x200029D0) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0000ms, 0670ms total)
T0F10 004:427 JLINK_ReadMemEx(0x200002A0, 0x0004 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(4 bytes @ 0x200002A0) - Data: 00 00 00 00  returns 0x04 (0000ms, 0670ms total)
T0F10 004:427 JLINK_ReadMemEx(0x20000E60, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x20000E60) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0001ms, 0671ms total)
T27A0 004:428 JLINK_IsHalted()  returns FALSE (0000ms, 0671ms total)
T27A0 004:529 JLINK_IsHalted()  returns FALSE (0000ms, 0671ms total)
T27A0 004:630 JLINK_IsHalted()  returns FALSE (0000ms, 0671ms total)
T27A0 004:731 JLINK_IsHalted()  returns FALSE (0000ms, 0671ms total)
T27A0 004:832 JLINK_IsHalted()  returns FALSE (0000ms, 0671ms total)
T27A0 004:933 JLINK_IsHalted()  returns FALSE (0000ms, 0671ms total)
T27A0 005:034 JLINK_ReadMemU32(0xE0001004, 0x0001 Items, ...) - Data: 4D CC 74 03  returns 1 (0000ms, 0671ms total)
T0F10 005:034 JLINK_ReadMemEx(0x200029D0, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x200029D0) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0000ms, 0671ms total)
T0F10 005:034 JLINK_ReadMemEx(0x200002A0, 0x0004 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(4 bytes @ 0x200002A0) - Data: 00 00 00 00  returns 0x04 (0001ms, 0672ms total)
T0F10 005:035 JLINK_ReadMemEx(0x20000E60, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x20000E60) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0000ms, 0672ms total)
T27A0 005:035 JLINK_IsHalted()  returns FALSE (0001ms, 0673ms total)
T27A0 005:137 JLINK_IsHalted()  returns FALSE (0000ms, 0672ms total)
T27A0 005:237 JLINK_IsHalted()  returns FALSE (0000ms, 0672ms total)
T27A0 005:338 JLINK_IsHalted()  returns FALSE (0000ms, 0672ms total)
T27A0 005:439 JLINK_IsHalted()  returns FALSE (0000ms, 0672ms total)
T27A0 005:540 JLINK_IsHalted()  returns FALSE (0000ms, 0672ms total)
T27A0 005:641 JLINK_ReadMemU32(0xE0001004, 0x0001 Items, ...) - Data: 4D CC 74 03  returns 1 (0000ms, 0672ms total)
T0F10 005:643 JLINK_ReadMemEx(0x200029D0, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x200029D0) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0001ms, 0673ms total)
T0F10 005:644 JLINK_ReadMemEx(0x200002A0, 0x0004 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(4 bytes @ 0x200002A0) - Data: 00 00 00 00  returns 0x04 (0001ms, 0674ms total)
T0F10 005:645 JLINK_ReadMemEx(0x20000E60, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x20000E60) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0000ms, 0674ms total)
T27A0 005:645 JLINK_IsHalted()  returns FALSE (0000ms, 0674ms total)
T27A0 005:746 JLINK_IsHalted()  returns FALSE (0000ms, 0674ms total)
T27A0 005:847 JLINK_IsHalted()  returns FALSE (0000ms, 0674ms total)
T27A0 005:948 JLINK_IsHalted()  returns FALSE (0000ms, 0674ms total)
T27A0 006:049 JLINK_IsHalted()  returns FALSE (0000ms, 0674ms total)
T27A0 006:150 JLINK_IsHalted()  returns FALSE (0000ms, 0674ms total)
T27A0 006:251 JLINK_ReadMemU32(0xE0001004, 0x0001 Items, ...) - Data: 4D CC 74 03  returns 1 (0000ms, 0674ms total)
T0F10 006:251 JLINK_ReadMemEx(0x200029D0, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x200029D0) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0000ms, 0674ms total)
T0F10 006:252 JLINK_ReadMemEx(0x200002A0, 0x0004 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(4 bytes @ 0x200002A0) - Data: 00 00 00 00  returns 0x04 (0000ms, 0674ms total)
T0F10 006:252 JLINK_ReadMemEx(0x20000E60, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x20000E60) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0001ms, 0675ms total)
T27A0 006:253 JLINK_IsHalted()  returns FALSE (0000ms, 0675ms total)
T27A0 006:354 JLINK_IsHalted()  returns FALSE (0000ms, 0675ms total)
T27A0 006:454 JLINK_IsHalted()  returns FALSE (0000ms, 0675ms total)
T27A0 006:556 JLINK_IsHalted()  returns FALSE (0000ms, 0675ms total)
T27A0 006:657 JLINK_IsHalted()  returns FALSE (0000ms, 0675ms total)
T27A0 006:758 JLINK_IsHalted()  returns FALSE (0000ms, 0675ms total)
T27A0 006:859 JLINK_ReadMemU32(0xE0001004, 0x0001 Items, ...) - Data: 4D CC 74 03  returns 1 (0000ms, 0675ms total)
T0F10 006:859 JLINK_ReadMemEx(0x200029D0, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x200029D0) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0000ms, 0675ms total)
T0F10 006:860 JLINK_ReadMemEx(0x200002A0, 0x0004 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(4 bytes @ 0x200002A0) - Data: 00 00 00 00  returns 0x04 (0001ms, 0676ms total)
T0F10 006:861 JLINK_ReadMemEx(0x20000E60, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x20000E60) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0000ms, 0676ms total)
T27A0 006:862 JLINK_IsHalted()  returns FALSE (0000ms, 0676ms total)
T27A0 006:963 JLINK_IsHalted()  returns FALSE (0000ms, 0676ms total)
T27A0 007:063 JLINK_IsHalted()  returns FALSE (0000ms, 0676ms total)
T27A0 007:164 JLINK_IsHalted()  returns FALSE (0000ms, 0676ms total)
T27A0 007:266 JLINK_IsHalted()  returns FALSE (0000ms, 0676ms total)
T27A0 007:367 JLINK_IsHalted()  returns FALSE (0000ms, 0676ms total)
T27A0 007:468 JLINK_ReadMemU32(0xE0001004, 0x0001 Items, ...) - Data: 4D CC 74 03  returns 1 (0000ms, 0676ms total)
T0F10 007:468 JLINK_ReadMemEx(0x200029D0, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x200029D0) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0000ms, 0676ms total)
T0F10 007:470 JLINK_ReadMemEx(0x200002A0, 0x0004 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(4 bytes @ 0x200002A0) - Data: 00 00 00 00  returns 0x04 (0000ms, 0676ms total)
T0F10 007:470 JLINK_ReadMemEx(0x20000E60, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x20000E60) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0001ms, 0677ms total)
T27A0 007:471 JLINK_IsHalted()  returns FALSE (0000ms, 0677ms total)
T27A0 007:573 JLINK_IsHalted()  returns FALSE (0000ms, 0677ms total)
T27A0 007:673 JLINK_IsHalted()  returns FALSE (0001ms, 0678ms total)
T27A0 007:775 JLINK_IsHalted()  returns FALSE (0000ms, 0677ms total)
T27A0 007:875 JLINK_IsHalted()  returns FALSE (0000ms, 0677ms total)
T27A0 007:976 JLINK_IsHalted()  returns FALSE (0000ms, 0677ms total)
T27A0 008:077 JLINK_ReadMemU32(0xE0001004, 0x0001 Items, ...) - Data: 4D CC 74 03  returns 1 (0000ms, 0677ms total)
T0F10 008:077 JLINK_ReadMemEx(0x200029D0, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x200029D0) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0000ms, 0677ms total)
T0F10 008:079 JLINK_ReadMemEx(0x200002A0, 0x0004 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(4 bytes @ 0x200002A0) - Data: 00 00 00 00  returns 0x04 (0001ms, 0678ms total)
T0F10 008:080 JLINK_ReadMemEx(0x20000E60, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x20000E60) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0000ms, 0678ms total)
T27A0 008:080 JLINK_IsHalted()  returns FALSE (0000ms, 0678ms total)
T27A0 008:181 JLINK_IsHalted()  returns FALSE (0000ms, 0678ms total)
T27A0 008:282 JLINK_IsHalted()  returns FALSE (0000ms, 0678ms total)
T27A0 008:384 JLINK_IsHalted()  returns FALSE (0000ms, 0678ms total)
T27A0 008:485 JLINK_IsHalted()  returns FALSE (0000ms, 0678ms total)
T27A0 008:586 JLINK_IsHalted()  returns FALSE (0000ms, 0678ms total)
T27A0 008:686 JLINK_ReadMemU32(0xE0001004, 0x0001 Items, ...) - Data: 4D CC 74 03  returns 1 (0000ms, 0678ms total)
T0F10 008:686 JLINK_ReadMemEx(0x200029D0, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x200029D0) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0000ms, 0678ms total)
T0F10 008:687 JLINK_ReadMemEx(0x200002A0, 0x0004 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(4 bytes @ 0x200002A0) - Data: 00 00 00 00  returns 0x04 (0001ms, 0679ms total)
T0F10 008:688 JLINK_ReadMemEx(0x20000E60, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x20000E60) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0000ms, 0679ms total)
T27A0 008:689 JLINK_IsHalted()  returns FALSE (0000ms, 0679ms total)
T27A0 008:790 JLINK_IsHalted()  returns FALSE (0000ms, 0679ms total)
T27A0 008:891 JLINK_IsHalted()  returns FALSE (0000ms, 0679ms total)
T27A0 008:992 JLINK_IsHalted()  returns FALSE (0000ms, 0679ms total)
T27A0 009:093 JLINK_IsHalted()  returns FALSE (0000ms, 0679ms total)
T27A0 009:194 JLINK_IsHalted()  returns FALSE (0000ms, 0679ms total)
T27A0 009:294 JLINK_ReadMemU32(0xE0001004, 0x0001 Items, ...) - Data: 4D CC 74 03  returns 1 (0000ms, 0679ms total)
T0F10 009:294 JLINK_ReadMemEx(0x200029D0, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x200029D0) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0002ms, 0681ms total)
T0F10 009:297 JLINK_ReadMemEx(0x200002A0, 0x0004 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(4 bytes @ 0x200002A0) - Data: 00 00 00 00  returns 0x04 (0001ms, 0682ms total)
T0F10 009:298 JLINK_ReadMemEx(0x20000E60, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x20000E60) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0000ms, 0682ms total)
T27A0 009:298 JLINK_IsHalted()  returns FALSE (0001ms, 0683ms total)
T27A0 009:400 JLINK_IsHalted()  returns FALSE (0000ms, 0682ms total)
T27A0 009:500 JLINK_IsHalted()  returns FALSE (0000ms, 0682ms total)
T27A0 009:601 JLINK_IsHalted()  returns FALSE (0000ms, 0682ms total)
T27A0 009:702 JLINK_IsHalted()  returns FALSE (0000ms, 0682ms total)
T27A0 009:802 JLINK_ReadMemU32(0xE0001004, 0x0001 Items, ...) - Data: 4D CC 74 03  returns 1 (0000ms, 0682ms total)
T0F10 009:802 JLINK_ReadMemEx(0x200029D0, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x200029D0) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0000ms, 0682ms total)
T0F10 009:803 JLINK_ReadMemEx(0x200002A0, 0x0004 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(4 bytes @ 0x200002A0) - Data: 00 00 00 00  returns 0x04 (0000ms, 0682ms total)
T0F10 009:804 JLINK_ReadMemEx(0x20000E60, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x20000E60) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0000ms, 0682ms total)
T27A0 009:804 JLINK_IsHalted()  returns FALSE (0000ms, 0682ms total)
T27A0 009:905 JLINK_IsHalted()  returns FALSE (0000ms, 0682ms total)
T27A0 010:006 JLINK_IsHalted()  returns FALSE (0000ms, 0682ms total)
T27A0 010:107 JLINK_IsHalted()  returns FALSE (0000ms, 0682ms total)
T27A0 010:208 JLINK_IsHalted()  returns FALSE (0000ms, 0682ms total)
T27A0 010:309 JLINK_IsHalted()  returns FALSE (0000ms, 0682ms total)
T27A0 010:410 JLINK_ReadMemU32(0xE0001004, 0x0001 Items, ...) - Data: 4D CC 74 03  returns 1 (0000ms, 0682ms total)
T0F10 010:410 JLINK_ReadMemEx(0x200029D0, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x200029D0) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0001ms, 0683ms total)
T0F10 010:411 JLINK_ReadMemEx(0x200002A0, 0x0004 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(4 bytes @ 0x200002A0) - Data: 00 00 00 00  returns 0x04 (0001ms, 0684ms total)
T0F10 010:412 JLINK_ReadMemEx(0x20000E60, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x20000E60) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0000ms, 0684ms total)
T27A0 010:412 JLINK_IsHalted()  returns FALSE (0001ms, 0685ms total)
T27A0 010:514 JLINK_IsHalted()  returns FALSE (0000ms, 0684ms total)
T27A0 010:615 JLINK_IsHalted()  returns FALSE (0000ms, 0684ms total)
T27A0 010:716 JLINK_IsHalted()  returns FALSE (0000ms, 0684ms total)
T27A0 010:818 JLINK_IsHalted()  returns FALSE (0000ms, 0684ms total)
T27A0 010:919 JLINK_IsHalted()  returns FALSE (0000ms, 0684ms total)
T27A0 011:019 JLINK_ReadMemU32(0xE0001004, 0x0001 Items, ...) - Data: 4D CC 74 03  returns 1 (0000ms, 0684ms total)
T0F10 011:019 JLINK_ReadMemEx(0x200029D0, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x200029D0) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0000ms, 0684ms total)
T0F10 011:020 JLINK_ReadMemEx(0x200002A0, 0x0004 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(4 bytes @ 0x200002A0) - Data: 00 00 00 00  returns 0x04 (0000ms, 0684ms total)
T0F10 011:020 JLINK_ReadMemEx(0x20000E60, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x20000E60) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0001ms, 0685ms total)
T27A0 011:021 JLINK_IsHalted()  returns FALSE (0000ms, 0685ms total)
T27A0 011:123 JLINK_IsHalted()  returns FALSE (0000ms, 0685ms total)
T27A0 011:224 JLINK_IsHalted()  returns FALSE (0000ms, 0685ms total)
T27A0 011:324 JLINK_IsHalted()  returns FALSE (0000ms, 0685ms total)
T27A0 011:425 JLINK_IsHalted()  returns FALSE (0000ms, 0685ms total)
T27A0 011:526 JLINK_IsHalted()  returns FALSE (0001ms, 0686ms total)
T27A0 011:627 JLINK_ReadMemU32(0xE0001004, 0x0001 Items, ...) - Data: 4D CC 74 03  returns 1 (0000ms, 0685ms total)
T0F10 011:627 JLINK_ReadMemEx(0x200029D0, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x200029D0) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0000ms, 0685ms total)
T0F10 011:629 JLINK_ReadMemEx(0x200002A0, 0x0004 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(4 bytes @ 0x200002A0) - Data: 00 00 00 00  returns 0x04 (0000ms, 0685ms total)
T0F10 011:629 JLINK_ReadMemEx(0x20000E60, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x20000E60) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0001ms, 0686ms total)
T27A0 011:630 JLINK_IsHalted()  returns FALSE (0000ms, 0686ms total)
T27A0 011:731 JLINK_IsHalted()  returns FALSE (0000ms, 0686ms total)
T27A0 011:832 JLINK_IsHalted()  returns FALSE (0000ms, 0686ms total)
T27A0 011:933 JLINK_IsHalted()  returns FALSE (0000ms, 0686ms total)
T27A0 012:034 JLINK_IsHalted()  returns FALSE (0000ms, 0686ms total)
T27A0 012:135 JLINK_IsHalted()  returns ERROR (0000ms, 0686ms total)
T27A0 012:135 JLINK_Halt()CPU could not be halted  returns 0x01 (0003ms, 0689ms total)
T27A0 012:138 JLINK_IsHalted()  returns ERROR (0001ms, 0690ms total)
T27A0 012:139 JLINK_IsHalted()  returns ERROR (0000ms, 0689ms total)
T27A0 012:139 JLINK_IsHalted()  returns ERROR (0000ms, 0689ms total)
T27A0 012:139 JLINK_ReadReg(R15 (PC)) -- CPU is running
  ***** Error: Can not read register 15 (R15) while CPU is running  returns 0x00000000 (0001ms, 0690ms total)
T27A0 012:140 JLINK_ReadReg(XPSR) -- CPU is running
  ***** Error: Can not read register 16 (XPSR) while CPU is running  returns 0x00000000 (0000ms, 0690ms total)
T27A0 012:140 JLINK_ReadMemU32(0xE000ED30, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000ED30)  returns -1 (0001ms, 0691ms total)
T27A0 012:141 JLINK_ReadReg(R0) -- CPU is running
  ***** Error: Can not read register 0 (R0) while CPU is running  returns 0x00000000 (0000ms, 0691ms total)
T27A0 012:141 JLINK_ReadReg(R1) -- CPU is running
  ***** Error: Can not read register 1 (R1) while CPU is running  returns 0x00000000 (0000ms, 0691ms total)
T27A0 012:142 JLINK_ReadReg(R2) -- CPU is running
  ***** Error: Can not read register 2 (R2) while CPU is running  returns 0x00000000 (0000ms, 0691ms total)
T27A0 012:142 JLINK_ReadReg(R3) -- CPU is running
  ***** Error: Can not read register 3 (R3) while CPU is running  returns 0x00000000 (0000ms, 0691ms total)
T27A0 012:142 JLINK_ReadReg(R4) -- CPU is running
  ***** Error: Can not read register 4 (R4) while CPU is running  returns 0x00000000 (0001ms, 0692ms total)
T27A0 012:143 JLINK_ReadReg(R5) -- CPU is running
  ***** Error: Can not read register 5 (R5) while CPU is running  returns 0x00000000 (0000ms, 0692ms total)
T27A0 012:143 JLINK_ReadReg(R6) -- CPU is running
  ***** Error: Can not read register 6 (R6) while CPU is running  returns 0x00000000 (0000ms, 0692ms total)
T27A0 012:143 JLINK_ReadReg(R7) -- CPU is running
  ***** Error: Can not read register 7 (R7) while CPU is running  returns 0x00000000 (0001ms, 0693ms total)
T27A0 012:144 JLINK_ReadReg(R8) -- CPU is running
  ***** Error: Can not read register 8 (R8) while CPU is running  returns 0x00000000 (0000ms, 0693ms total)
T27A0 012:144 JLINK_ReadReg(R9) -- CPU is running
  ***** Error: Can not read register 9 (R9) while CPU is running  returns 0x00000000 (0001ms, 0694ms total)
T27A0 012:145 JLINK_ReadReg(R10) -- CPU is running
  ***** Error: Can not read register 10 (R10) while CPU is running  returns 0x00000000 (0000ms, 0694ms total)
T27A0 012:145 JLINK_ReadReg(R11) -- CPU is running
  ***** Error: Can not read register 11 (R11) while CPU is running  returns 0x00000000 (0000ms, 0694ms total)
T27A0 012:145 JLINK_ReadReg(R12) -- CPU is running
  ***** Error: Can not read register 12 (R12) while CPU is running  returns 0x00000000 (0001ms, 0695ms total)
T27A0 012:146 JLINK_ReadReg(R13 (SP)) -- CPU is running
  ***** Error: Can not read register 13 (R13) while CPU is running  returns 0x00000000 (0000ms, 0695ms total)
T27A0 012:146 JLINK_ReadReg(R14) -- CPU is running
  ***** Error: Can not read register 14 (R14) while CPU is running  returns 0x00000000 (0000ms, 0695ms total)
T27A0 012:146 JLINK_ReadReg(R15 (PC)) -- CPU is running
  ***** Error: Can not read register 15 (R15) while CPU is running  returns 0x00000000 (0000ms, 0695ms total)
T27A0 012:146 JLINK_ReadReg(XPSR) -- CPU is running
  ***** Error: Can not read register 16 (XPSR) while CPU is running  returns 0x00000000 (0001ms, 0696ms total)
T27A0 012:147 JLINK_ReadReg(MSP) -- CPU is running
  ***** Error: Can not read register 17 (MSP) while CPU is running  returns 0x00000000 (0000ms, 0696ms total)
T27A0 012:147 JLINK_ReadReg(PSP) -- CPU is running
  ***** Error: Can not read register 18 (PSP) while CPU is running  returns 0x00000000 (0000ms, 0696ms total)
T27A0 012:147 JLINK_ReadReg(CFBP) -- CPU is running
  ***** Error: Can not read register 20 (CFBP) while CPU is running  returns 0x00000000 (0001ms, 0697ms total)
T27A0 012:148 JLINK_ReadReg(FPSCR) -- CPU is running
  ***** Error: Can not read register 32 (FPSCR) while CPU is running  returns 0x00000000 (0000ms, 0697ms total)
T27A0 012:148 JLINK_ReadReg(FPS0) -- CPU is running
  ***** Error: Can not read register 33 (FPS0) while CPU is running  returns 0x00000000 (0000ms, 0697ms total)
T27A0 012:148 JLINK_ReadReg(FPS1) -- CPU is running
  ***** Error: Can not read register 34 (FPS1) while CPU is running  returns 0x00000000 (0001ms, 0698ms total)
T27A0 012:149 JLINK_ReadReg(FPS2) -- CPU is running
  ***** Error: Can not read register 35 (FPS2) while CPU is running  returns 0x00000000 (0000ms, 0698ms total)
T27A0 012:149 JLINK_ReadReg(FPS3) -- CPU is running
  ***** Error: Can not read register 36 (FPS3) while CPU is running  returns 0x00000000 (0000ms, 0698ms total)
T27A0 012:149 JLINK_ReadReg(FPS4) -- CPU is running
  ***** Error: Can not read register 37 (FPS4) while CPU is running  returns 0x00000000 (0001ms, 0699ms total)
T27A0 012:150 JLINK_ReadReg(FPS5) -- CPU is running
  ***** Error: Can not read register 38 (FPS5) while CPU is running  returns 0x00000000 (0000ms, 0699ms total)
T27A0 012:150 JLINK_ReadReg(FPS6) -- CPU is running
  ***** Error: Can not read register 39 (FPS6) while CPU is running  returns 0x00000000 (0001ms, 0700ms total)
T27A0 012:151 JLINK_ReadReg(FPS7) -- CPU is running
  ***** Error: Can not read register 40 (FPS7) while CPU is running  returns 0x00000000 (0000ms, 0700ms total)
T27A0 012:151 JLINK_ReadReg(FPS8) -- CPU is running
  ***** Error: Can not read register 41 (FPS8) while CPU is running  returns 0x00000000 (0000ms, 0700ms total)
T27A0 012:151 JLINK_ReadReg(FPS9) -- CPU is running
  ***** Error: Can not read register 42 (FPS9) while CPU is running  returns 0x00000000 (0001ms, 0701ms total)
T27A0 012:152 JLINK_ReadReg(FPS10) -- CPU is running
  ***** Error: Can not read register 43 (FPS10) while CPU is running  returns 0x00000000 (0000ms, 0701ms total)
T27A0 012:152 JLINK_ReadReg(FPS11) -- CPU is running
  ***** Error: Can not read register 44 (FPS11) while CPU is running  returns 0x00000000 (0000ms, 0701ms total)
T27A0 012:152 JLINK_ReadReg(FPS12) -- CPU is running
  ***** Error: Can not read register 45 (FPS12) while CPU is running  returns 0x00000000 (0001ms, 0702ms total)
T27A0 012:153 JLINK_ReadReg(FPS13) -- CPU is running
  ***** Error: Can not read register 46 (FPS13) while CPU is running  returns 0x00000000 (0000ms, 0702ms total)
T27A0 012:153 JLINK_ReadReg(FPS14) -- CPU is running
  ***** Error: Can not read register 47 (FPS14) while CPU is running  returns 0x00000000 (0000ms, 0702ms total)
T27A0 012:153 JLINK_ReadReg(FPS15) -- CPU is running
  ***** Error: Can not read register 48 (FPS15) while CPU is running  returns 0x00000000 (0000ms, 0702ms total)
T27A0 012:153 JLINK_ReadReg(FPS16) -- CPU is running
  ***** Error: Can not read register 49 (FPS16) while CPU is running  returns 0x00000000 (0001ms, 0703ms total)
T27A0 012:154 JLINK_ReadReg(FPS17) -- CPU is running
  ***** Error: Can not read register 50 (FPS17) while CPU is running  returns 0x00000000 (0000ms, 0703ms total)
T27A0 012:154 JLINK_ReadReg(FPS18) -- CPU is running
  ***** Error: Can not read register 51 (FPS18) while CPU is running  returns 0x00000000 (0001ms, 0704ms total)
T27A0 012:155 JLINK_ReadReg(FPS19) -- CPU is running
  ***** Error: Can not read register 52 (FPS19) while CPU is running  returns 0x00000000 (0000ms, 0704ms total)
T27A0 012:155 JLINK_ReadReg(FPS20) -- CPU is running
  ***** Error: Can not read register 53 (FPS20) while CPU is running  returns 0x00000000 (0000ms, 0704ms total)
T27A0 012:155 JLINK_ReadReg(FPS21) -- CPU is running
  ***** Error: Can not read register 54 (FPS21) while CPU is running  returns 0x00000000 (0001ms, 0705ms total)
T27A0 012:156 JLINK_ReadReg(FPS22) -- CPU is running
  ***** Error: Can not read register 55 (FPS22) while CPU is running  returns 0x00000000 (0000ms, 0705ms total)
T27A0 012:156 JLINK_ReadReg(FPS23) -- CPU is running
  ***** Error: Can not read register 56 (FPS23) while CPU is running  returns 0x00000000 (0000ms, 0705ms total)
T27A0 012:157 JLINK_ReadReg(FPS24) -- CPU is running
  ***** Error: Can not read register 57 (FPS24) while CPU is running  returns 0x00000000 (0000ms, 0705ms total)
T27A0 012:157 JLINK_ReadReg(FPS25) -- CPU is running
  ***** Error: Can not read register 58 (FPS25) while CPU is running  returns 0x00000000 (0001ms, 0706ms total)
T27A0 012:158 JLINK_ReadReg(FPS26) -- CPU is running
  ***** Error: Can not read register 59 (FPS26) while CPU is running  returns 0x00000000 (0000ms, 0706ms total)
T27A0 012:158 JLINK_ReadReg(FPS27) -- CPU is running
  ***** Error: Can not read register 60 (FPS27) while CPU is running  returns 0x00000000 (0000ms, 0706ms total)
T27A0 012:158 JLINK_ReadReg(FPS28) -- CPU is running
  ***** Error: Can not read register 61 (FPS28) while CPU is running  returns 0x00000000 (0001ms, 0707ms total)
T27A0 012:159 JLINK_ReadReg(FPS29) -- CPU is running
  ***** Error: Can not read register 62 (FPS29) while CPU is running  returns 0x00000000 (0000ms, 0707ms total)
T27A0 012:159 JLINK_ReadReg(FPS30) -- CPU is running
  ***** Error: Can not read register 63 (FPS30) while CPU is running  returns 0x00000000 (0000ms, 0707ms total)
T27A0 012:159 JLINK_ReadReg(FPS31) -- CPU is running
  ***** Error: Can not read register 64 (FPS31) while CPU is running  returns 0x00000000 (0001ms, 0708ms total)
T0F10 012:160 JLINK_ReadMemEx(0x200029D0, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x200029D0) - Data: AA AA AA AA AA AA AA AA AA AA AA AA AA AA AA AA ...  returns 0xFFFFFFFF (0000ms, 0708ms total)
T0F10 012:161 JLINK_ReadMemEx(0x200002A0, 0x0004 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(4 bytes @ 0x200002A0) - Data: AA AA AA AA  returns 0xFFFFFFFF (0000ms, 0708ms total)
T0F10 012:162 JLINK_ReadMemEx(0x20000E60, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x20000E60) - Data: AA AA AA AA AA AA AA AA AA AA AA AA AA AA AA AA ...  returns 0xFFFFFFFF (0000ms, 0708ms total)
T0F10 012:162 JLINK_ReadMemEx(0x00000000, 0x003C Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(4 bytes @ 0x40023844) -- CPU_ReadMem(60 bytes @ 0x08000000) - Data: AA AA AA AA AA AA AA AA AA AA AA AA AA AA AA AA ...  returns 0xFFFFFFFF (0001ms, 0709ms total)
T0F10 012:163 JLINK_ReadMemEx(0x00000000, 0x003C Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(60 bytes @ 0x08000000) - Data: AA AA AA AA AA AA AA AA AA AA AA AA AA AA AA AA ...  returns 0xFFFFFFFF (0000ms, 0709ms total)
T0F10 012:163 JLINK_ReadMemEx(0x00000000, 0x003C Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(60 bytes @ 0x08000000) - Data: AA AA AA AA AA AA AA AA AA AA AA AA AA AA AA AA ...  returns 0xFFFFFFFF (0001ms, 0710ms total)
T0F10 012:164 JLINK_ReadMemEx(0x00000002, 0x0002 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(2 bytes @ 0x08000002) - Data: AA AA  returns 0xFFFFFFFF (0000ms, 0710ms total)
T0F10 012:164 JLINK_ReadMemEx(0x00000002, 0x0002 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(2 bytes @ 0x08000002) - Data: AA AA  returns 0xFFFFFFFF (0000ms, 0710ms total)
T0F10 012:164 JLINK_ReadMemEx(0x00000002, 0x0002 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(2 bytes @ 0x08000002) - Data: AA AA  returns 0xFFFFFFFF (0001ms, 0711ms total)
T0F10 012:165 JLINK_ReadMemEx(0x00000004, 0x003C Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(60 bytes @ 0x08000004) - Data: AA AA AA AA AA AA AA AA AA AA AA AA AA AA AA AA ...  returns 0xFFFFFFFF (0000ms, 0711ms total)
T0F10 012:165 JLINK_ReadMemEx(0x00000004, 0x003C Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(60 bytes @ 0x08000004) - Data: AA AA AA AA AA AA AA AA AA AA AA AA AA AA AA AA ...  returns 0xFFFFFFFF (0001ms, 0712ms total)
T0F10 012:166 JLINK_ReadMemEx(0x00000004, 0x003C Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(60 bytes @ 0x08000004) - Data: AA AA AA AA AA AA AA AA AA AA AA AA AA AA AA AA ...  returns 0xFFFFFFFF (0001ms, 0713ms total)
T3E34 012:166 
  ***** Error: Connection to emulator lost! (1597ms, 2310ms total)
T3E34 012:166 
  ***** Error: Connection to emulator lost! (417970ms, 418683ms total)
T3E34 012:166 
  ***** Error: Connection to emulator lost! (1738670ms, 1739383ms total)
T0F10 60097:214 JLINK_Close() (0009ms, 0722ms total)
T0F10 60097:214  (0009ms, 0722ms total)
T0F10 60097:214 Closed (0009ms, 0722ms total)
