{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["SheetJS"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"SheetJS","index":0,"n_rows":10,"n_cols":14,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
["牧场","安全阀类型","安全阀型号","公称通径","公称压力MPa","工作压力MPa","整定压力MPa","起跳压力MPa","回座压力MPa","使用位置","使用部门","本次检验日期","下次检验日期","管理责任人"]
["宝鸡牧场","弹簧式安全阀","A48Y-16Q","50MM",1.6,0.6,0.8,0.85,0.72,"沼气锅炉","能源处","2019-05-31","2020-05-30","王立宝"]
["宝鸡牧场","弹簧式安全阀","A48Y-16Q","50MM",1.6,0.6,0.8,0.85,0.72,"沼气锅炉","能源处","2019-05-31","2020-05-30","王立宝"]
["宝鸡牧场","弹簧式安全阀","A47Y-16Q","50MM",1.6,0.73,0.8,0.85,0.72,"分气缸","能源处","2019-04-01","2020-03-31","王立宝"]
["宝鸡牧场","弹簧式安全阀","A47Y-16Q","40MM",1.6,0.6,0.8,0.8,0.72,"换热器","能源处","2019-04-01","2020-03-31","王立宝"]
["宝鸡牧场","弹簧式安全阀","A48Y-16C","80MM",1.6,1.01,1.07,1.07,0.85,"1#燃煤锅炉","设备处","2019-09-28","2020-09-27","任孔军"]
["宝鸡牧场","弹簧式安全阀","A48Y-16C","80MM",1.6,1.01,1.07,1.07,0.85,"1#燃煤锅炉","设备处","2019-09-28","2020-09-27","任孔军"]
["宝鸡牧场","弹簧式安全阀","A48Y-16C","80MM",1.6,1.01,1.07,1.07,0.85,"2#燃煤锅炉","设备处","2019-09-28","2020-09-27","任孔军"]
["宝鸡牧场","弹簧式安全阀","A48Y-16C","80MM",1.6,1.01,1.07,1.07,0.85,"2#燃煤锅炉","设备处","2019-09-28","2020-09-27","任孔军"]
["宝鸡牧场","弹簧式安全阀","A48Y-16C","50MM",1.6,0.91,1,1,0.85,"换热器","设备处","2019-09-28","2020-09-27","任孔军"]